T
SECTION 105100
 (New SECTION 105113)

LOCKERS
(74000, 75000 & 76000)

Display hidden notes to specifier. (Don't know how? Click Here) 

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	12-inch Wide Four-Tier Vented Metal Lockers
B.	12-inch Wide Five-Tier Box Style Vented Metal Lockers.
C.	12-inch Wide Six-Tier Box Style Vented Metal Lockers.

1.2	REFERENCES

A.	IBC - International Building Code.

1.3	RELATED SECTIONS
	
A.	Section 03300 (03 30 00) – Cast-in-Place Concrete:  Concrete bases.
B.	Section 06100 (06 10 00) – Rough Carpentry:  Wood ground and furring for anchoring lockers.
C.	Section 09650 (09 65 13.13) – Resilient Base.

1.4	SUBMITTALS
A.	Submit under provisions of Section 013300.
B.	Product Data - Manufacturer's data sheets on each product to be used, including:
1.	Preparation instructions and recommendations.
2.	Storage and handling requirements and recommendations.
3.	Installation methods.
C.	Shop Drawings:  Prepared specifically for this project; show dimensions of lockers and interface with other products.
D.	Selection Samples:  For each finish product specified, two complete sets of color chips representing manufacturer's full range of available colors and patterns. . 

1.5	QUALITY ASSURANCE
A.	Manufacturer Qualifications:  Manufacturer shall have a Quality System in place to ensure and be able to substantiate that manufactured units conform to requirements and match the approved design and must be ISO 9001:2015 certified.

1.6	DELIVERY, STORAGE, AND HANDLING
A.	Store products in manufacturer's unopened packaging until ready for installation.
B.	Locker components shall be stored flat, if shipped unassembled, until assembly. All finishes shall be protected from soiling and damage during handling.
C.	Store and dispose of solvent-based materials, and materials used with solvent-based materials, in accordance with requirements of local authorities having jurisdiction.

1.7	WARRANTY
A.	Manufacturer's standard warranty to repair or replace components of locker products that fail in materials or workmanship within 3 years from date of Substantial Completion.

PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Salsbury Industries, 18300 Central Avenue, Carson, CA 90746-4008; Toll Free Telephone: 1-800-LOCKERS (1-800-562-5377); Fax: 1-800-562-5399; Email: salsbury@lockers.com; Website: www.lockers.com.
B.	Substitutions:  Not permitted.

2.2	LOCKERS
12-inch wide vented metal lockers:  Constructed of 16 gauge steel; durable powder coated finish; features a strong steel hasp; can accommodate built-in combination locks, built-in key locks, combination padlocks, key padlocks, factory installed resettable combination locks or factory installed electronic combination locks.

A.	12-inch Wide Vented Metal Locker Series:
1.	74000 series:  Four-tier.
2.	75000 series:  Five-tier Box Style.
3.	76000 series:  Six-tier Box Style.

B.	Unit Width: 12 inches (305 mm).

C.	Unit Height:	
		1.	5 feet Lockers: 
a.	66 inches (1,676 mm) with legs.
b.	64 inches (1,626mm) with zee base.
c.	60 inches (1,524 mm) without legs.
		2.	6 feet Lockers:
a.	78 inches (1,981 mm) with legs.
b.	76 inches (1,930 mm) with zee base.
c.	72 inches (1,828 mm) without legs.

D.	Unit Depth: 
1.	12 inches (305 mm).
		2.	15 inches (381 mm).
		3.	18 inches (457 mm).
	
E.	Unit Assembly: 
1.	Unassembled units (Knocked-down).
		2.	Assembled units.

F.	Unit Color: 
1.	Color: Gray - standard.
	2.	Color: Tan - standard.
	3.	Color: Blue - standard.

2.3	OPTIONAL EQUIPMENT

A.	Sloping hoods.

B.	Base panels – 6 inches (152 mm) high: 
1.	Front base.
	2.	End base.

C.	Fillers: 
1.	Flat top fillers:
			a.	Flat top in-line top fillers.
		b.	Flat top corner fillers.
	2.	Sloping hood fillers:
		a.	Sloping in-line top fillers.
		b.	Sloping corner fillers.
	3.	Front fillers:
		a.	9 inch (229 mm) wide filler panels.
		b.	15 inch (381 mm) wide filler panels.

D.	Finished end panels: 
1.	Single end panel for end of unit rows.
	2.	Double end panel for back-to-back unit installations.

E.	Built-In Locks: 
1.	Built-in combination locks.
	2.	Built-in keyed locks.
	3.	Factory installed resettable combination locks.
	4.	Factory installed electronic combination locks.

F.	Padlocks:
	1.	Combination padlocks.
	2.	Keyed padlocks.

G.	Master keys: 
1.	Master control key for built-in combination locks.
	2.	Master control key for built-in keyed locks.
	3.	Master control key for combination padlocks.
	
H.	Engraved name/number plates. 

I.	Locker unit legs shall be supplied, unless otherwise specified, at 6 inches (152 mm) high in same color as locker unit.  Locker bases shall be fabricated from 0.0625 inch (1.59 mm) thick steel sheet.
J.	Locker zee base kit – 4 inches (102 mm) high by 72 inches (1828 mm) in length in same color as locker unit.  Locker zee base kits shall be fabricated from 0.0625 inch (1.59 mm) thick steel sheet.

		1.	12 inches (305 mm).
		2.	15 inches (381 mm).
		3.	18 inches (457 mm).
K.	Lockers without legs.

		1.	12 inches (305 mm).
		2.	15 inches (381 mm).
		3.	18 inches (457 mm).
	
L.	Anchoring Brackets - For use in lockers without legs.

2.4	CONSTRUCTION
A.	Locker Doors:  Steel specially formed for added strength and rigidity and to ensure tight joints at fastening points. 
1.	Door:
a.  16 gauge - .060 inch (1.52 mm) thick steel.
		b.  Holes provided for attaching number plates.
2.	Ventilation:  1-1/2 inch (38 mm) wide by 3/4 inch (19 mm) high diamond-shaped perforations.
3.	Hasp:  16-gauge steel hasp with padlock attachment, when not used 		with built-in locks.
B.	Locker Body:  Solid steel specially formed for added strength and rigidity and to ensure tight joints at fastening points.
C.	Hinges:  Hinge: 0.074 inch (1.88 mm) thick sheet steel, double spun, full loop, tight pin, projection welded to door frame and securely fastened to the door. 
1.	Hinge:  Two 2 inch (51 mm) high five-knuckle hinges.
D.	Optional factory assembly of locker bodies using heavy duty steel rivets.

PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until substrates have been properly prepared.
B.	If substrate preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.

3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.

3.3	INSTALLATION
A.	Install in accordance with Salsbury Industries’ installation instructions.
B.	Anchor the units to the wall studs through the locker back and to the floor.
C.	Lockers can be either floor-mounted or installed on concrete or wood bases as scheduled or indicated.  Floor or base shall be level for proper installation.

3.4	PROTECTION
A.	Protect installed products until completion of project.
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION