SECTION 105100
 (New SECTION 105123)

LOCKERS
(31000, 32000, 33000, 34000, 35000, 36000, 37000)

Display hidden notes to specifier. (Don't know how? Click Here) 

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	12-inch Wide Single-Tier Designer Wood Lockers.
B.	12-inch Wide Double-Tier Designer Wood Lockers.
C.	12-inch Wide Double-Tier S-Style Designer Wood Lockers.
D.	12-inch Wide Triple-Tier Designer Wood Lockers.
E.	12-inch Wide Four-Tier Designer Wood Lockers.
F.	12-inch Wide Five-Tier Box-Style Designer Wood Lockers.
G	12-inch Wide Six-Tier Box-Style Designer Wood Lockers.

1.2	REFERENCES
A.	ADAAG - Americans with Disabilities Act, Accessibility Guidelines.
B.	IBC - International Building Code.
C.	LEED Submittal Requirements NC v3.0:  Sustainable Design Requirements – LEED for New Construction and the LEED NC v3.0 reference guide.

1.3	RELATED SECTIONS
A.	Section 06114 - Wood Blocking and Curbing; Wood grounds and attachment strips.
B.	Section 06200 - Finish Carpentry:  Related trim not specified in this section.

1.4	SUBMITTALS
A.	Product Data:  Manufacturer's data sheets on each product to be used, including:
1.	Preparation instructions and recommendations.
2.	Storage and handling requirements and recommendations.
3.	Installation methods.
B.	Shop Drawings:  Prepared specifically for this project; show dimensions of lockers and interface with other products.
C.	Selection Samples:  For each finish product specified, two complete sets of color chips representing manufacturer's full range of available colors and patterns.
D.	Submit under provisions of LEED NC v3.0 reference guide:  Product data for each type of accessory specified, with installation instructions for each unit built-in or connected to other construction:
1.	Product Data for Credit MR 4 – Recycled Content:  For products having recycled content, documentation indicating percentages by weight of post-consumer and pre-consumer recycled content.
2.	Product Data for Credit MR 5 – Regional Materials:  Provide documentation indicating where materials have been extracted, harvested or recovered, as well as manufactured.  If only a portion of the product has been extracted, harvested or recovered, and manufactured within 500 miles of the job site, then indicate that percentage.
3.	Product Data for IEQ 4.1 – Low Emitting Materials-Adhesives and Sealants:  Provide documentation including printed statement of VOC content for all adhesives and sealants.
4.	Product Data for Credit IEQ 4.2:   Submit product data and MSDS for interior paints and coatings, verifying VOC levels and compliance for Green Seal Standard GS-11, GC-03 and SCAQMD Rule 1113.
5.	Laboratory Test Reports for Credit IEQ 4.2:  For primers, documentation indicating that products comply with the testing and product requirements of the California Department of Health Services’ “Standard Practice for the Testing of Volatile Organic Emissions from Various Sources Using Small-Scale Environmental Chambers”.

1.5 	QUALITY ASSURANCE
A.	Manufacturer Qualifications:  Manufacturer shall have a Quality System in place to ensure and be able to substantiate that manufactured units conform to requirements and match the approved design and must be ISO 9001:2015 certified.

1.6	DELIVERY, STORAGE, AND HANDLING
A.	Store products in manufacturer's unopened packaging, in a dry, ventilated area until ready for installation.
B.	Locker components shall be stored flat, if shipped unassembled, until assembly. All finishes shall be protected from soiling and damage during handling.
C.	Store and dispose of solvent-based materials, and materials used with solvent-based materials, in accordance with requirements of local authorities having jurisdiction.

1.7	WARRANTY
A.	Manufacturer's standard warranty to repair or replace components of locker products that fail in materials or workmanship within 3 years from date of Substantial Completion.

PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Salsbury Industries, 18300 Central Avenue, Carson, CA 90746-4008; Toll Free Tel: 800-LOCKERS (800-562-5377); Fax: 800-562-5399; Email: salsbury@lockers.com; Website: www.lockers.com. 
B.	Substitutions:  Not permitted. 

2.2	LOCKERS
Single-tier, double-tier, double-tier s-style, triple-tier, four-tier, five-tier box style and six-tier box style 12-inch wide designer wood lockers:  Constructed of industrial grade particleboard and covered with durable plastic laminate; includes a lift up handle and recessed hasp for added security; can accommodate built-in combination or key locks, combination or key padlocks, resettable combination locks or electronic locks.  Lockers are available as fully assembled units only and require minor assembly.

A.	12-inch Wide Designer Wood Locker Series:
1.	31000 series:  Single-tier.
2.	32000 series:  Double-tier.
3.	33000 series:  Triple-tier.
4.	34000 series:  Four-tier.
5.	35000 series:  Five-tier Box style.
6.	36000 series:  Six-tier Box style.
7.	37000 series:  Double-tier S-style.

B.	Unit Width:  12 inches (304 mm).

C.	Unit Height:
1.	5 foot locker units:
a.	64 inches (1,626 mm) with bases.
b.	60 inches (1,524 mm) without bases.
2.	6 foot locker units:
a.	76 inches (1,930 mm) with bases.
b.	72 inches (1,828 mm) without bases.

D.	Unit Depth:
1.	15 inches (381 mm).
2.	18 inches (457 mm).
		3.	21 inches (533 mm).

E.	Unit Assembly:  Requires minor assembly.

F.	Laminate Color: 
1.	Color: Gray - standard.
2.	Color: Blue - standard.
	3.	Color: Black - standard.
	4.	Color: Maple - standard.
	5.	Color: Cherry - standard.
	6.	Color: Mahogany - standard.

2.3	INTERIOR EQUIPMENT

A.	ADA Compliant Lockers (Recessed Handles with Multi-Point Latch):
1.	Single-tier, double-tier, and triple-tier lockers:  						Additional shelf at maximum 48 inches (1,219 mm) off the floor for 			unobstructed forward and side reach. 
2.	Handicapped Locker Compartment Bottom:  Minimum of 15 inches (381 mm) off the floor or an extra shelf placed 15 inches (381 mm) off the floor for unobstructed forward and side reach.
3.	Hooks and rods as specified.

B.	Standard Hardware Features: 
1.	Single Tier Designer Wood Lockers:
			a.	Padlock hasp.
			b.	One top-mounted, two-pronged stainless steel coat hook.
			c.	One full depth hat shelf.
			d.	One 5 inch (127 mm) deep shelf.
			e.	One 11-3/4 inch (298 mm) deep shoe shelf.
			f.	Three heavy duty concealed door hinges.
2.	Double Tier, Double Tier S-Style and Triple Tier Designer Wood Lockers:
			a.	Padlock hasp.
			b.	One top-mounted, two-pronged stainless steel coat hook.
			c.	One 5 inch (127 mm) deep shelf.
			d.	Two heavy duty concealed door hinges.
	3.	Four Tier and Box Style Lockers:
a.	Packlock hasp.
b.	Two heavy duty concealed door hinges.

2.4	OPTIONAL EQUIPMENT

	A.	Sloping hoods:
		1.	12 inches (305 mm) for 1-wide units.
		2.	36 inches (914 mm) for 3-wide units.

B.	Bases:  4 inches (102 mm) high.

C.	Fillers:
	1.	Flat top fillers:
		a.	Flat top in-line top fillers.
		b.	Flat top corner fillers.
	2.	Sloping hood fillers:
		a.	Sloping In-line top fillers.
		b.	Sloping corner fillers.
	3.	Front fillers:
		a.	9 inch (229 mm) wide filler panels.
		b.	15 inch (381 mm) wide filler panels.
		c.	Vertical corner fillers.

D.	Side panels:
	1.	Single end side panels:
		a.	Without sloping hoods.
		b.	With sloping hoods.
	2.	Double end side panels:
		a.	Without sloping hoods.
		b.	With sloping hoods.

E.	Built-In Locks:
	1.	Built-in combination locks.
	2.	Built-in keyed locks.
	3.	Built-in resettable combination locks.
	4.	Built-in electronic locks.

F.	Padlocks:
	1.	Combination padlocks.
	2.	Keyed padlocks.

G.	Master keys:
	1.	Master control key for built-in combination locks.
	2.	Master control key for built-in keyed locks.
	3.	Master control key for built-in resettable combination locks.
	4.	Master control key for combination padlocks.

H.	Additional compartment shelf.

I.	Engraved name/number plates.

2.5	CUSTOMIZATION

A.	Custom colors – For all custom colors available, contact Salsbury Industries or visit www.lockers.com/customdesignerlockers:
	1.	Minimum order of ten locker frames.

	B.	Ventilation grill:  Improved air flow throughout locker compartment.

C.	Coat rod:  Additional garment storage capability.

D.	Visibility window:  Polycarbonate window to view locker contents.

E.	Lockers without doors:  Easy storage access.

F.	Lockable interior compartment:  Add protection for items.

2.6	CONSTRUCTION
A.	Locker Body – Tops, bottoms, sides, backs and shelves are precision machined:
1.	Locker shall be fabricated using doweled and glued assembly process.
2. 	Tops and bottoms with three sides formed to 90 degrees, the front offset formed to be flush with horizontal frame member.
3.	Shelves with four sides formed to 90 degrees.

B.	Locker Doors – Doors are precision machined: 
1.	Door:
		a.	Doors have four radial edges.
		b.	Routed inset to insert and attach number plates.
2.	Ventilation – 1/2 inch (12.7 mm) opening between door and frame on locker top and bottom provide unrestricted airflow:
a.	Customizable venting option available.
3.	Single-point latching:
			a.	Recessed handle in door.
			b.	Integral Pocket and Pull:  22 gauge powder coated stainless 					steel securely fastened to door with two lugs and a positive 					tamper-resistant decorative fastener.
I.	Pocket Depth:  Sufficient to prevent a combination padlock,
built-in combination lock, or key lock from protruding beyond door face.
				II.	Pull:  Formed in pocket.
				III.	Padlock Staple:  Protruding through pocket.
			c.	Provide lock hole cover plate for use with padlocks.
			d.	Locking Device:  11 gauge steel hasp welded to locker frame; 					include surface for engaging the bolt of a built-in combination 					or key lock and anti-pry lug and slot to deter prying open when locked.
			e.	Firmly secure rubber silencers to locker frame.
C.	Fabricate locker parts square, rigid and without warp, with the finished faces flat and free of scratches and chips.
D.	Fabricate corners and fillers as required for installation.

PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until substrates have been properly prepared.
B.	If substrate preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.

3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.

3.3	INSTALLATION
A.	Install in accordance with Salsbury Industry's installation instructions.
B.	Anchor the units to the wall studs through the locker back and to the floor.
C.	Lockers can be either floor-mounted or installed on concrete or wood bases as scheduled or indicated.  Floor or base shall be level for proper installation.

3.4	PROTECTION
A.	Protect installed products until completion of project.
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION