SECTION 105100
 (New SECTION 105153)

LOCKER BENCHES
(77780D, 77781D, 77782D)

Display hidden notes to specifier. (Don't know how? Click Here) 

PART 1    GENERAL
1.1	SECTION INCLUDES
A.	Designer Wood Locker Benches.
B.	Designer Wood ADA Locker Benches.

1.2	REFERENCES
A.	ADAAG - Americans with Disabilities Act, Accessibility Guidelines.
B.	IBC - International Building Code.
C.	LEED Submittal Requirements NC v3.0:  Sustainable Design Requirements – LEED for New Construction and the LEED NC v3.0 reference guide.

1.3	SUBMITTALS
A.	Product Data:  Manufacturer's data sheets on each product to be used, including:
1.	Preparation instructions and recommendations.
2.	Storage and handling requirements and recommendations.
3.	Installation methods.
B.	Shop Drawings:  Prepared specifically for this project; show dimensions of lockers and interface with other products.
C.	Selection Samples:  For each finish product specified, two complete sets of color chips representing manufacturer's full range of available colors and patterns.
D.	Submit under provisions of LEED NC v3.0 reference guide:  Product data for each type of accessory specified, with installation instructions for each unit built-in or connected to other construction:
1.	Product Data for Credit MR 4 – Recycled Content:  For products having recycled content, documentation indicating percentages by weight of post-consumer and pre-consumer recycled content.
2.	Product Data for Credit MR 5 – Regional Materials:  Provide documentation indicating where materials have been extracted, harvested or recovered, as well as manufactured.  If only a portion of the product has been extracted, harvested or recovered, and manufactured within 500 miles of the job site, then indicate that percentage.
3.	Product Data for IEQ 4.1 – Low Emitting Materials-Adhesives and Sealants:  Provide documentation including printed statement of VOC content for all adhesives and sealants.
4.	Product Data for Credit IEQ 4.2:   Submit product data and MSDS for interior paints and coatings, verifying VOC levels and compliance for Green Seal Standard GS-11, GC-03 and SCAQMD Rule 1113.
5.	Laboratory Test Reports for Credit IEQ 4.2:  For primers, documentation indicating that products comply with the testing and product requirements of the California Department of Health Services’ “Standard Practice for the Testing of Volatile Organic Emissions from Various Sources Using Small-Scale Environmental Chambers”.

1.4	QUALITY ASSURANCE
A.	Manufacturer Qualifications:  Manufacturer shall have a Quality System in place to ensure and be able to substantiate that manufactured units conform to requirements and match the approved design and must be ISO 9001:2015 certified.

1.5	DELIVERY, STORAGE, AND HANDLING
A.	Store products in manufacturer's unopened packaging, in a dry, ventilated area until ready for installation.
B.	Locker components shall be stored flat, if shipped unassembled, until assembly. All finishes shall be protected from soiling and damage during handling.
C.	Store and dispose of solvent-based materials, and materials used with solvent-based materials, in accordance with requirements of local authorities having jurisdiction.

1.6	WARRANTY
A.	Manufacturer's standard warranty to repair or replace components of locker products that fail in materials or workmanship within 3 years from date of Substantial Completion.

PART 2    PRODUCTS
2.1	MANUFACTURERS
A.	Acceptable Manufacturer: Salsbury Industries, 18300 Central Avenue, Carson, CA 90746-4008; Toll Free Tel: 800-LOCKERS (800-562-5377); Fax: 800-562-5399; Email: salsbury@lockers.com; Website: www.lockers.com. 
B.	Substitutions:  Not permitted. 

2.2	LOCKERS
Standard and ADA-compliant designer wood locker benches:  Constructed of industrial grade particleboard and covered with durable high pressure plastic laminate; includes two 3 inch (76 mm) diameter bolt mounted pedestals in a black powder coated finish; pedestals include four (4) mounting holes to secure to the ground; combines a classic look with strength and durability. Requires minor assembly.

A.	Designer Wood Locker Bench Series:
1.	77783D:  36” Wide (914 mm) Wood Locker Bench.
2.	77784D:  48” Wide (1,219 mm) Wood Locker Bench.
3.	77785D:  60” Wide (1,524 mm) Wood Locker Bench.
4.	77786D:  72” Wide (1,829 mm) Wood Locker Bench.
5.	77787D:  84” Wide (2,134 mm) Wood Locker Bench.
6	77788D:  96” Wide (2,438 mm) Wood Locker Bench.
7.	77781D-ADA:  42” Wide (1,067 mm) Wood ADA Locker Bench.
8.	77781D-ADAB:  42” Wide (1,067 mm) Wood ADA Locker Bench					with Back Support.
9.	77782D-ADA:  48” Wide (1,219 mm) Wood ADA Locker Bench.
10.	77782D-ADAB:  48” Wide (1,219 mm) Wood ADA Locker Bench					with Back Support.

A.	Unit Heights:
1.	77783D, 77784D, 77785D, 77786D, 77787D, 77788D:
a.	18 inches (457 mm).
2.	77781D-ADA & 77782D-ADA:
a.	18 inches (457 mm).
3.	77781D-ADAB & 77782D-ADAB:
a.	18 inches (457 mm) seat height.
b.	39 inches (991 mm) back support height.

C.	Unit Depth:
1.	77783D, 77784D, 77785D, 77786D, 77787D, 77788D:
a.	9.5 inches (241 mm).
2.	77781D-ADA & 77782-ADA:
a.	20 inches (508 mm).
3.	77781D-ADAB & 77782D-ADAB:
a.	20 inches (508 mm) seat depth.
b.	23 inches (584 mm) back support depth.

D.	Unit Assembly:  Requires minor assembly.

E.	Laminate Color: 
1.	Color: Gray - standard.
2.	Color: Blue - standard.
	3.	Color: Black - standard.
	4.	Color: Maple - standard.
	5.	Color: Cherry - standard.
	6.	Color: Mahogany - standard.

2.5	CONSTRUCTION
A.	Locker Bench – Seating area:
1.	Shall be made of industrial grade particleboard and covered with	durable high pressure plastic laminate
2. 	All corners to have radial edges.
3.	Side surfaces shall be sealed with black rubber banding.

B.	Bench Pedestals:
1.	Pedestals shall consist of aluminum tubing, 3 inches (76 mm) in diameter.
2.	Base shall be ¼” (6 mm) thick aluminum welded to each end of aluminum tubing.
3.	Finished in black powder coat.
C.	Fabricate locker bench parts square, rigid and without warp, with the finished faces flat and free of scratches and chips.

PART 3    EXECUTION
3.1	EXAMINATION
A.	Do not begin installation until substrates have been properly prepared.
B.	If substrate preparation is the responsibility of another installer, notify Architect of unsatisfactory preparation before proceeding.

3.2	PREPARATION
A.	Clean surfaces thoroughly prior to installation.
B.	Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions.

3.3	INSTALLATION
A.	Install in accordance with Salsbury Industry's installation instructions.
B.	Anchor the units to the floor through the bench pedestal’s holes:
	1.	Standard bench pedestals:  Four (4) holes.
	2.	ADA-compliant bench pedestals:  Two (2) holes.
C.	Locker benches can be either floor-mounted or installed on concrete or wood bases as scheduled or indicated.  Floor or base shall be level for proper installation.

3.4	PROTECTION
A.	Protect installed products until completion of project.
B.	Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION